**Tender List, Lot No. \_\_\_**

1. **Name of Goods, works, services:** supply of equipment for transportation of bottles and cullet return and packaging in pallets line 5.4.
2. **Method of conducting the trade procedure:** RFQ
3. **Address of delivery of Goods, works, services:** 8a, Dargomyzhskogo, Novosibirsk, Russia
4. **Condition of delivery of Goods, work, services (terms, schedules, packaging, labeling):**

* Terms of supply – DAP Novosibirsk

Packaging of Goods must ensure the safety of the goods during transportation by any kind of transport.

1. **Form, terms and procedure of payment for goods, work, services. The procedure for the formation of the contract price (lot price) (including or excluding transportation costs, insurance, payment of customs duties, taxes and other mandatory payments):** 50% advance payment; 50% after the signing of the act of acceptance of products in the warehouse of the buyer.

The supplier provides a cost calculation broken down by equipment units

1. **Information about the initial (maximum) contract price (lot price):** not defined
2. **Technical requirements for manufacturing technology, design, materials:** according to the Design Documentation (DD) СК-3.16.05.000ТП

To accept for initial data. The performance lines for the production of:

ЭБ4-П-62-100 Стакан 0,1л (Appendix №1) – at least 540 units per minute

Э715-ВДП-3Э-250 Костровок 0,25 л (Appendix №2) - at least 540 units per minute

Э437N-И-В-203-330 «Шейк-1» (Appendix №3) – 540 at least 540 units per minute

1. **Quantity of goods, scope of work, volume of services:**

|  |  |  |  |
| --- | --- | --- | --- |
| **№ п/п** | **Name of equipment** | **Unit** | **кол-во** |
| 1 | Conveyer from Lehr | kit | 1 |
| 2 | Cascade Conveyer | kit | 1 |
| 3 | Conveyer empty bottles | kit | 1 |
| 4 | Angle Conveyer | kit | 1 |
| 5 | Accumulation table (reversible) | kit | 1 |
| 6 | Palletizer | kit | 1 |
| 7 | Conveyer cullet | kit | 1 |

1. **Requirements to the package bundle:** conveyer empty bottles, Conveyer from Lehr, Cascade Conveyer must be equipped with drive gear motors, plate conveyor chains, straight and rotary, corresponding to the width of the products, conveyor sides, substrates for conveyor chains, corresponding to the type of chains. Reverse cullet conveyor must also be equipped with a gear motor and a conveyor belt of the appropriate type. The palletizer shall have automatic supply of wooden pallets, gaskets and boxes, possibility of installation of inflatable captures from 27 to 110 mm.
2. **Requirements to the quality:** according to the requirements of the manufacturer
3. **Requirements for installation, commissioning, acceptance tests:** The supplier performs installation supervision and commissioning.
4. **Requirements for manufacturer's warranty and after-sales service conditions:**

the supplier provides a guarantee for the equipment for a period of 24 months from the date of exploitation start

1. **Ranking criteria of participants of the procurement procedure (minimum delivery price, minimum delivery time, other criteria):**

* minimal quotation price.
* Applicants who have provided with the offer signed on their part the original contracts (by mail) or scans, ceteris paribus will have an advantage in ranking or selection the winner.

1. **Requirements to participants of the procurement procedure and the list of documents submitted by participants of the procurement procedure to confirm their compliance with the established requirements:** Reference list over the past 5-10 years

**Appendices:**

1. Appendix №1
2. Appendix №2
3. Appendix №3
4. Design Documentation СК-3.16.05.000ТП