**Tender List, Lot No.\_\_\_\_**

1. **Name of Goods, works, services:** supply of equipment for the operation of the process control system of the glass melting furnace №5
2. **Method of conducting the trade procedure:** simple purchase
3. **Address of delivery of Goods, works, services:**  **:** Sibsteklo LLC**,** 8a, Dargomyzhskogo, Novosibirsk, Russia
4. **Condition of delivery of Goods, work, services (terms, schedules, packaging, labeling):**

* delivery time is not more than 4 months from the date of payment of the advance;
* terms of delivery DAP Novosibirsk.

Packaging of Goods must ensure the safety of the goods during transportation by any kind of transport.

1. **Form, terms and procedure of payment for goods, work, services. The procedure for the formation of the contract price (lot price) (including or excluding transportation costs, insurance, payment of customs duties, taxes and other mandatory payments):**

The buyer makes payment for the products to the Supplier within 15 calendar days from the date of signing by the parties of invoices and receiving an invoice by transferring the relevant amounts to the Supplier’s current account by the Buyer

1. **Information about the initial (maximum) contract price (lot price):** not defined
2. **Technical requirements for manufacturing technology, design, materials:** according to the Technical Requirements for the implementation of the modernization of the control system of the furnace number 5 K-21 (Appendix No. 1 to Tender list)
3. **Quantity of goods, scope of work, volume of services:** According to clauses 7.5, 9.2, 9.3 of the Technical Requirements for the execution of works on the modernization of the control system of the furnace No. 5 К-21 (Appendix No. 1 to Tender list
4. **Requirements to the package bundle:** according to Technical requirements (Appendix 1 to Tender list).
5. **Requirements to the quality:** according to the requirements of the manufacturer.
6. **Requirements for installation, commissioning, acceptance tests:** Supplier performs installation supervision at the agreed additional term.
7. **Requirements for manufacturer's warranty and after-sales service conditions:**

The warranty period for the delivered equipment is 24 months after the completion of commissioning, achievement of the required indicators from the date of signing of the Act of executed works.

1. **Ranking criteria of participants of the procurement procedure (minimum delivery price, minimum delivery time, other criteria):**

* minimal quotation price.

1. **Requirements to participants of the procurement procedure and the list of documents submitted by participants of the procurement procedure to confirm their compliance with the established requirements:** Reference list
2. Appendix to Tender list:

- Technical requirements for projection of distributor including 4 feeders of Glass Furnace No. 5 at building 21;

- The contract for the supply of equipment to ensure the operation of the process control system of the glass melting furnace No. 5;